Product Date sheet

**Linear** **series**



**IP20**

**TECHNICAL** **DRAWINGS**



Product Code: Linear series

**DESIGN** **BY**

Emilux architecture

**DESCRIPTION**

Opal lighting for general use and outlining

Average lighting on opal cover

Average performance within differernt length

External dimming interface withTriac,0/1-10V,Dali

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **FEATURES**  Article Code:  Colour:  Installation:  Environment:  **GENERAL** **SPECIFICATION** | | Linear series  Black/White  Magnetic  Indoor | | |
| CCT:  CRI:  LED:  DIM: | 2700K/3000K/4000K  RA90  OSRAM  Triac,0/1-10V,Dali | | | |
| **AVAILABLE** **MODELS** | | | | |
| Item Power(w) Size(mm) | | | | |
| EM-S20F4-10W 10W L300\*W22\*H45mm | | | | |
| EM-S20F4-20W | 20W | L600\*W22\*H45mm | | |
| EM-S20F4-30W | 30W | L900\*W22\*H45mm | | |
| EM-S20F4-40W | 40W | L1200\*W22\*H45mm | | |
| **PACKAGE** **INFORMATION** | | | | |
| Item Qty/Ctn(pcs) N.W/Ctn(kgs) G.W/Ctn(kgs) L\*W\*H(cm) | | | | |
| EM-S20F4-10W 20 5.7 7.5 44.5x22.24 | | | | |
| EM-S20F4-20W | 20 | 9.8 | 12.2 | 44.5x38x28 | |
| EM-S20F4-30W | 10 | 9.1 | 11.7 | 70x18.5x35 | |
| EM-S20F4-40W | 10 | 14 | 16.3 | 101x17.5x36 | |
| **LIGHT** **DISTRIBUTION** | | | | |

